**SAFETY CHECK**

1. CIRCUIT BREAKERS CLOSED
2. N/W STRG SWITCH OFF
3. HYDRAULIC PUMPS OFF
4. LDG GEAR LEVER DN / DOWN
5. FLIGHT SPOILER LEVER RETRACTED
6. SLATS / FLAPS LEVER SET
7. RADAR OFF
8. ADG MANUAL RELEASE STOWED
9. EMER FLAP SWITCH NORMAL
10. BATTERY MASTER SWITCH ON
11. APU ON/OFF
12. AC ELECTRICS AS REQUIRED
13. IRS NAV
14. EMERGENCY EQUIPMENT CHECKED
15. GEAR AND SAFETY PINS ON BOARD
16. AIRPLANE DOCUMENTS CHECKED
17. HYDRAULIC 3A PUMP ON/OFF
18. FMS INITIALIZATION COMPLETE

**CABIN INSPECTION & EXTERNAL WALKAROUND**

1. CABIN INSPECTION ACCOMPLISH
2. WALKAROUND INSPECTION ACCOMPLISH

**ORIGINATING CHECK**

1. CREW OXYGEN AND MASKS CHECKED / \_\_\_\_\_PSI

ONLY FIRST FLIGHT OF THE DAY

1. AUDIO WARNING PANEL CHECKED
2. ELECTRICAL POWER PANEL CHECKED
3. FIRE DETECTION / FIREX MONITOR TEST COMPLETE  
   ONLY FIRST FLIGHT OF THE DAY
4. EXTERNAL LIGHTS PANEL CHECKED
5. FUEL PANEL CHECKED
6. BLEED AIR PANEL CHECKED
7. APU PANEL ON/OFF
8. START PANEL CHECKED
9. HYDRAULIC PANEL CHECKED, AUTO,ON (3A)
10. ELT SWITCH ARM / RESET
11. CABIN PRESS PANEL CHECKED
12. AIR CONDITIONING PANEL CHECKED
13. ANTI-ICE PANEL CHECKED, COMPLETE
14. WSHLD HEAT LOW
15. EMER LTS SWITCH ARMED
16. STANDBY COMPASS CHECKED
17. N/W STRG SWITCH OFF
18. CLOCKS SET
19. INSTRUMENT PANELS CHECKED
20. UPPER PEDESTAL CHECKED
21. THRUST LEVER QUADRANT CHECKED
22. AVIONICS / RADIO TUNING PANELS CHECKED
23. TRIMS CHECKED
24. YAW DAMPER ENGAGE
25. SOURCE SELECT PANEL NORM

**BEFORE START CHECK**

1. PASS SIGNS ON
2. LDG ELEV SET
3. ALTIMETERS \_\_,\_\_\_ FEET
4. FMS CHECKED, SET
5. IRS ALIGNED, NAV
6. RADIOS AND NAV AIDS SET
7. TAKE-OFF BRIEFING COMPLETE

**CLEARED TO START CHECK**

1. PERSONAL ELECTRONIC DEV. OFF
2. APU ON
3. ELECTRICS CHECKED
4. TAKE-OFF DATA SET
5. DOORS CLOSED / LOCKED
6. BEACON ON
7. FUEL PUMPS AND QUANTITY ON, \_\_\_\_\_\_\_\_\_\_kg/lbs
8. HYDRAULIC PUMPS AUTO / ON
9. PARKING BRAKE ON/OFF

**AFTER START CHECK**

1. GENERATORS AUTO
2. ELECTRICS CHECKED
3. BLEED VALVES AUTO
4. PACKS ON
5. APU ON/OFF
6. ANTI-ICE ON/OFF
7. N/W STRG ARMED

**TAXI CHECK**

1. SLATS / FLAPS \_\_\_ ° INDICATING
2. FLIGHT CONTROLS CHECKED
3. TRIMS GREEN & \_\_\_\_ UNITS
4. THRUST REVERSERS ARMED
5. FLIGHT INSTRUMENTS CHECKED
6. BRAKE TEMP CHECKED

**BEFORE TAKE-OFF CHECK**

1. LIGHTS AND STROBES ON
2. FUEL, XFLOW MANUAL
3. FLIGHT ATTENDANT ADVISED
4. TRANSPONDER / TCAS ON, SET
5. RADAR / TERRAIN DISPLAY SET
6. CAS CHECKED

**CLIMB CHECK**

1. FUEL, XLFOW AUTO
2. BLEEDS AND APU SET
3. THRUST REVERSERS OFF
4. CAS CHECKED

**DESCENT CHECK**

1. LDG ELEV SET
2. FUEL CHECKED
3. TCAS SET
4. RADAR ON/OFF
5. CAS CHECKED
6. LANDING DATA SET
7. APPROACH BRIEFING COMPLETE

**BEFORE LANDING CHECK**

1. FLIGHT ATTENDANT ADVISED
2. PASS SIGNS ON
3. THRUST REVERSERS ARMED
4. LDG GEAR DOWN
5. FLAPS \_\_\_ ° INDICATING

**AFTER LANDING CHECK**

1. APU ON/OFF
2. TRANSPONDER / RADAR STBY / OFF
3. FLAPS UP / ZERO
4. LIGHTS AND STROBES SET
5. PROBES OFF

**SHUTDOWN CHECK**

1. PARKING BRAKE ON/OFF
2. SEAT BELTS OFF
3. THRUST LEVERS SHUT OFF
4. ANTI ICE OFF
5. FUEL PUMPS OFF
6. BEACON OFF
7. N/W STRG SWITCH OFF

**TERMINATING CHECK**

1. CHOCKS AND BRAKES IN / OFF
2. IRS OFF
3. EMER LTS SWITCH OFF
4. ANTI-ICE OFF
5. HYDRAULIC PUMPS OFF
6. EXTERNAL LTS SWITCHES OFF
7. APU OFF
8. BATTERY MASTER OFF
9. COCKPIT LIGHTS OFF